*DOUBTS*

1. If we want one LED in **active-high** way (**Initially OFF**), we would do:

DDRB = DDRB | (1 <<LED)

PORTB = PORTB &~ (1<<LED)

Right?

1. If we want one LED in **active-high** way (**Initially ON**), we would do:

DDRB = DDRB | (1 <<LED)

PORTB = PORTB | (1<<LED)

Right?

1. If we want one LED in **active-low** way (**Initially OFF**), we would do:

DDRB = DDRB | (1 <<LED)

PORTB = PORTB | (1<<LED)

Right?

1. If we want one LED in **active-low** way (**Initially ON**), we would do:

DDRB = DDRB | (1 <<LED)

PORTB = PORTB &~ (1<<LED)

Right?

1. With this lines, we would configure push-button in **active-low** way and **active-high** way, respectively:

DDRB = DDRB &~ (1 <<BTN) DDRB = DDRB &~ (1 <<BTN)

PORTB = PORTB | (1<<BTN) PORTB = PORTB &~ (1<<BTN)

Right?